PART 1: GENERAL

1.1 SECTION INCLUDES

A. Porcelain-on-Steel Markerboards.

B. Porcelain-on-Steel Chalkboards.

C. Colored Cork Tackboards.

D. Visual Display Board Accessories.

1.2 RELATED SECTIONS

A. Section 06100 – Wood or Steel Blocking.

B. Section 09000 – Gypsum Wall Board.

C. Section 09720 – Vinyl Wall Coverings.

D. Section 09900 – Paints and Coatings.

1.3 REFERENCES

A. ASTM B221 – Standard Specification for Aluminum and Aluminum-Alloy Extruded Bars, Rods, Wire, Shapes, and Tubes.

B. ASTM E84 –Test Method for Surface Burning and Characteristics of Building Materials.

C. ASTM C540 – Gloss Test for Porcelain Enamel Steel (Porcelain Enamel Institute PEI-501).

1.4 SUBMITTALS

A. Submit products and samples under provisions of Section 01300.

B. Product Data: Provide technical data for products specified. Include Material Safety Data Sheets, when applicable.

C. Shop Drawings: Provide shop drawings for each type of visual display board specified including section details

indicating trim, face, core and backing materials, dimensions, joint locations and special anchor details.

D. Color Samples: Submit set of color chips displaying manufacturer’s full range of colors and finishes.

E. Product Samples: Submit samples not less than twelve inches square and framed on two adjacent sides, to illustrate materials, finish, color, and configuration of each type of visual display board required.

1.5 DELIVERY, STORAGE AND HANDLING

A. Comply with manufacturer’s instructions for handling and storage of Visual Display Boards.

1.6 PROJECT CONDITIONS

A. Field measure prior to fabrication to ensure proper fit.

B. General contractor to maintain proper climate before, during and after installation.

1.7 WARRANTY

A. Submit manufacturer’s “Life of Building” warranty, stating that under normal usage and maintenance, and when

installed in accordance with manufacturer’s instructions and recommendations, Porcelain-on-Steel Markerboards and Chalkboards are guaranteed for the life of the building.

B. Warranty shall cover replacement of defective Porcelain-on-Steel Markerboards and Chalkboards due to

discoloration, excessive fading of color, crazing, cracking or flaking. Warranty does not cover the cost of removal or

reinstallation.

PART 2: PRODUCTS

2.1 MANUFACTURERS

A. Provide visual display boards as manufactured by Platinum Visual Systems™, Corona, California.

Tel.: (800)498-2990 Fax: (951)817-9900. Email: info@pvsusa.com. Website: www.pvsusa.com.

B. Substitutions: See Section 01600 – Product Requirements.

2.2 MARKERBOARD AND CHALKBOARD MATERIALS

A. Steel Face Sheets: Writing surface will be Writanium® 28 gauge steel face with porcelain enamel finish fused to the steel sheet using a continuous coil process.

1. Markerboard and Chalkboard surface shall be fused at a temperature of 1450º and 1200º, respectively.

2. The gloss of the writing surface will not increase more than three units when subjected to wearability tests specified in testing procedures for 30 hours.

B. Core Material: 1/2" particleboard.

C. Backing Material: .005" aluminum backing sheet.

D. Metal Trim and Accessories: 6063 aluminum alloy with a T5 temper.

E. Adhesive: As recommended by manufacturer for project conditions.

2.3 PORCELAIN-ON-STEEL MARKERBOARDS AND CHALKBOARDS

A. Provide Markerboards and Chalkboards for project from manufacturer’s MTS Series.

1. Metal trim and accessories: MTS Series aluminum extrusions with clear satin anodized finish.

a. Chalktray CR315: Standard continuous solid chalktray with ribbed section and smoothly curved and polished ends.

b. Map Rail MR411: Standard 1" high continuous rail with colored cork insert as follows:

1) End stops: One pair per Map Rail.

2) Map hooks: One every 2' of Map Rail.

3) Roller brackets: One pair per Map Rail.

4) Flag holder: One per room.

c. Frame CH210: Standard channel frame with 3/4" face with wrap around corners and miters.

d. Wall Standards: Single ST100 or Double ST200 punched with 3/8" x 1" slot 2" on center. Standards to be installed exactly 4'-0" on center. Height to be 72", 84" or 96" high.

e. Locking Device LD100: Spring loaded locking installed in upper corners of board.

2. Size: Available sizes 4' high x 4' wide or 4' high x 8' wide as shown on drawings.

3. Color: As selected from manufacturer’s standard colors.

2.4 COLORED CORK TACKBOARD MATERIALS

A. Face Sheet: Colored cork surface will be 1/4” resilient homogenous tackable linoleum surface consisting of linseed oil, granulated cork, rosin binders and dry pigments calendared onto natural burlap backing. Color shall extend through thickness of material and be self-healing.

B. Core Material: 1/4” medium density fiberboard.

C. Metal Trim: 6063 aluminum alloy with T5 temper.

D. Adhesive: As recommended by manufacturer for project conditions.

2.5 COLORED CORK TACKBOARDS

A. Provide Tackboards for project from manufacturer’s MTS Series.

1. Metal trim and accessories: MTS Series aluminum extrusions with clear satin anodized finish.

a. Frame CH210: Standard channel frame with 3/4" face with wrap around corners and miters.

b. Wall Standards: Single ST100 and Double ST200 punched with 3/8" x 1" slot 2" on center. Standards to be installed exactly 4'-0" on center. Height to be 72", 84" or 96" high.

c. Locking Device LD100: Spring loaded locking installed in upper corners of board.

2. Size: As shown on drawings.

3. Color: As selected from manufacturer’s standard colors.

2.6 FABRICATION

A. Laminate facing sheet and backing sheet to core material under pressure, using manufacturer’s recommended adhesive.

B. Assemble units in one piece without joints, wherever possible. Where required dimensions exceed maximum panel

size available, provide two or more pieces of equal length, as indicated on approved shop drawings. Assemble to verify fit at factory, then disassemble for delivery and final assembly at project site.

PART 3: EXECUTION

3.1 EXAMINATION

A. Verify that substrates are properly prepared to receive visual display boards. Do not begin installation until

unsatisfactory conditions have been corrected.

3.2 INSTALLATION

A. Comply with manufacturer’s installation instructions.

B. Where visual display boards must be partly assembled at project site, use factory-supplied H-bar to maintain

proper alignment.

C. Install visual display boards level and plumb, keeping perimeter trim aligned in accordance with manufacturer’s

recommendations.

3.3 ADJUSTING AND CLEANING

A. Verify that all accessories are installed as required for each unit.

B. Upon completion of installation, clean surfaces and trim in accordance with manufacturer’s recommendations,

leaving all materials ready for use.